{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BCC"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BCC","index":0,"n_rows":4,"n_cols":10,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,1,9]]}
["蒸汽裂解装置现场液位计检修完工检查确认清单\n检查要求：\n1.外观检查：液位计外观检查无明显瑕疵,设备完整良好；仪表位号牌齐全。现场检查符合要求的，在“外观检查”项中打”✔“，不符合打“×”。\n2.安装检查：液位计回装位置正确。现场检查符合要求的，在“安装检查”项中打”✔“，不符合打“×”。\n3.功能检查：液位计已经校验或清洗测试完成，功能完好；一次阀已经投用，具备使用条件。现场检查符合要求的，在“功能检查”项中打”✔“，不符合打“×”。\n以上检查中不符合要求的，必须按照该条检查内容的要求立即整改。如不能立即整改的，请立即汇报相关负责人并采取临时应对措施。"]
[]
["序号","单元号","液位计位号","外观检查","安装检查","功能检查","确认人1","确认人2","确认时间","备注"]
[1]