{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BCC"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BCC","index":0,"n_rows":6,"n_cols":15,"rows_kept":6,"cut":false,"hidden":false,"merged":[[2,14,3,14],[10,0,10,14],[0,0,1,14],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,2,10],[2,11,3,11],[2,12,3,12],[2,13,3,13]]}
["爆破片检查表\n检查要求：\n1、查看爆破片的安装位置是否正确，是（✔），否（×）,不符合要求的，立即联系相关责任人按照要求进行整改;\n2、检查爆破片的安装方向是否正确，是否投用，是（✔），否（×），不符合要求的，立即联系相关责任人按照要求进行整改;\n3、检查爆破片铭牌上压力和设定压力是否一致，是（✔），否（×），不符合要求的，立即联系相关责任人按照要求进行整改;\n4、查看爆破片与安全阀之间的压力指示是否为0kpa，是（✔），否（×）；0kpa为正常，如果超过0kpa则视为异常，立即联系相关责任人按照要求进行整改。"]
[]
["序号 ","单元号","位号","保护设备","\n安装位置\n描述","检查项目 ",{"$nulls":5},"检查人1","检查人2","检查日期","备注"]
[null,null,null,"管端",null,"爆破片的安装位置正确（是/否）","爆破片的安装方向正确（是/否）","投用\n（是/否）","设定压力\n（MPag）","铭牌上压力和\n设定压力一致\n（是/否）","爆破片与安全阀之间的压力指示为“0kpa”\n（是/否）"]
[1]
[{"$nulls":10}," "]